- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Windows / Power Window Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Power Windows / Power Window Switch Repair procedures

Inspection

Power Window Main Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim. (Refer to Body - "Front Door Trim")

3. | Disconnect the connector (A) from the power window switch module.

4. | Check for continuity between the terminals in each switch position according to the table. [Driver/Assist Safety] [Driver Auto Down]

Assist Power Window Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim panel. (Refer to Body - "Front Door Trim")

3. | Disconnect the connector (A) from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [Safety] [Manual]

Rear Power Window Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim panel. (Refer to Body - "Rear Door Trim")

3. | Disconnect the connector (A) from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [With Seat Heater] [Without Seat Heater]

Removal

Driver Power Window Switch

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim. (Refer to Body - "Front Door Trim")

3. | Remove the power window switch assembly (A) by loosening the mounting screws (8EA).

4. | Remove the power window switch assembly (A) after loosening the mounting screws.

Assist Power Window Switch

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim. (Refer to Body - "Front Door Trim")

3. | Remove the power window switch assembly (A) by loosening the mounting screws (7EA).

4. | Remove the power window switch assembly (A) after loosening the mounting screws.

Rear Power Window Swtich

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

3. | Remove the power window switch assembly (A) by loosening the mounting screws (7EA).

4. | Remove the power window switch assembly (A) after loosening the mounting screws.

Installation

Driver Power Window Switch

1. | Install the power window switch assembly.

2. | Install the front door trim after connecting the connector.

Assist Power Window Switch

1. | Install the power window switch assembly.

2. | Install the front door trim after connecting the connector.

Rear Power Window Swtich

1. | Install the power window switch assembly.

2. | Install the front door trim after connecting the connector.

##### Power Window Switch Schematic Diagrams

Circuit Diagram Driver Power Window Switch Assist Power Window Switch Rear Power Window Switch ...

##### Power Window Relay Repair procedures

Inspection Diagnosis With GDS 1. It can quickly diagnose defects of power window by communicating with GDS. GDS can operate actuator forcefully, monitor input/output values and self diagnose. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Console Armrest Components and Components Location

Component Location 1. Console armrest ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Photo Sensor Description and Operation

Description The photo sensor is located at the center of the defrost nozzles. The photo sensor contains a photovoltaic (sensitive to sunlight) diode. The solar radiation received by its light receiving portion, generates an electromotive force in proportion to the amount of radiation rece ...
Copyright © www.ksoulev.com 2020-2021