- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: BCM (Body Control Module) / Components and Components Location

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / BCM (Body Control Module) / Components and Components Location

Components

Connector Pin Information

No. | Connector A (24 pin) | Connector B (20 pin) | Connector C (26 pin) | Connector D (16 pin)
1 | Battery (+) | LIN (PAS) | Washer motor power | -
2 | IGN 1 | Fuel filler (Charge door) actuator relay | Front washer motor | -
3 | IGN 2 | LS CAN high | - | -
4 | Brake switch | LS CAN low | Mirror unfold relay | Mirror unfold switch
5 | Wiper mist switch | Mood lamp unlock state | DRL lamp LH | Mirror fold switch
6 | Crash unlock input (PWM) | Horn relay | DRL lamp RH | -
7 | - | - | Room lamp | -
8 | Fuel filler (Charge door) open switch | HS CAN low | - | -
9 | Wiper washer switch | HS CAN high | - | Auto light switch
10 | Wiper INT switch | Ground (Auot light) | - | Defogger switch
11 | Wiper low switch | Auto light signal | - | -
12 | Rear washer switch | Auto light power | Wiper low relay | Head lamp high switch
13 | ACC | Safety power window enable high | - | Head lamp low switch
14 | Wiper high switch | - | DRL lamp power | -
15 | Front fog lamp switch | ATM solenoid | Rear washer motor | -
16 | Rear wiper switch | - | Mirror fold relay | -
17 | Rear INT switch | Fuel filler (Charge door) lamp | MTS Tx | ?
18 | - | - | -
19 | - | - | Head lamp low signal
20 | - | Ground (Power) | AV tail
21 | Tail switch | ? | Wiper high relay
22 | Wiper INT volume | -
23 | LIN (Intelligent Battery Sensor) | -
24 | Ground (Signal) | -
25 | ? | -
26 | Ground (Power)

##### Specifications

Specifications ItemsSpecificationsRated voltageDC 12VOperating voltageDC 9 ~ 16VOperating temperature-30°C ~ 80°C (-4°F ~ 176°F)Dark currentBCM & Receiver : Max. 4 mABCM : Max. 3 mA ...

##### Description and Operation

Description BCM CAN Communication Function FunctionDescriptionTimerDefrosterWhen IGN ON, Rear Heater Control FunctionSafety Power WindowAccording to the position of key, Power Window Output C ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Hub / Knuckle Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) Be careful not to da ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Photo Sensor Description and Operation

Description The photo sensor is located at the center of the defrost nozzles. The photo sensor contains a photovoltaic (sensitive to sunlight) diode. The solar radiation received by its light receiving portion, generates an electromotive force in proportion to the amount of radiation rece ...
Copyright © www.ksoulev.com 2020-2021