- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Seat Electrical / Seat Heater Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Seat Electrical / Seat Heater Switch Repair procedures

Removal

First Row Seat

1. | Remove the heater & A/C control unit. (Refer to Heating, Ventilation And Air Conditioning - "Heater & A/C Control Unit (FATC)")

Second Row Seat

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

3. | Remove the power window switch assembly (A) by loosening the mounting screws (7EA).

Installation

First Row Seat

1. | Install the heater & A/C control unit. (Refer to Heating, Ventilation And Air Conditioning - "Heater & A/C Control Unit (FATC)")

Second Row Seat

1. | Install the power window switch.

2. | Install the rear door trim.

3. | Connect the negative (-) battery terminal.

Inspection

First Row Seat

1. | Disconnect the negative (-) batttery terminal.

2. | Disconnect the A/C & heater controller connectors (A). (Refer to Heating, Ventilation And Air Conditioning - "Heater & A/C Control Unit (FATC)")

3. | Operate switch and check for continuity between the terminals. If there is no continuity, replace the seat heater switch.

Second Row Seat

1. | Disconnect the negative (-) batttery terminal.

2. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

3. | Operate driver seat heater switch and check for continuity between the terminals. If there is no continuity, replace the seat heater switch.

##### Seat Heater Switch Schematic Diagrams

Circuit Diagram [First Row Seat] Second Row Seat ...

##### Seat Heater (Non-Air Ventilation) Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Roller Blind Repair procedures

Removal 1. Open the roller blind using the panorama sunroof switch. • Leave 10 ~ 20cm (0.3937 ~ 0.7874 in) of the roller blind unopened. 2. Remove the roof trim. (Refer to Roof Trim - "Roof Trim Assembly") 3. Remove the roller blind bar (C) by ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Current Sensor Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Prcedure") 3. Remove the high voltage battery system assembly. (Refer to High Voltage Battery System - Repair procedures - "Removal") 4. Remove the hi ...
Copyright © www.ksoulev.com 2020-2021