- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Suspension System / Power Electric Frame Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Front Suspension System / Power Electric Frame Repair procedures

Removal

1. | Remove the motor & gear drive unit. (Refer to Traction Motor System - "Motor & Gear Differential Unit Assembly")

2. | Remove the Electric Water Pump (EWP). (Refer to Traction Motor System - "Electric Water Pump")

3. | Remove the accumulator mounting bolt (A).
Tightening torque : 6.8 ~ 10.7 N.m(0.7 ~ 1.1 kgf.m, 5.0 ~ 7.9 lb-ft)

4. | Remove the wiring (A) from the power electric frame.

5. | Remove the LH & RH support bracket mounting nut (A,B) and then remove the Power Electric Frame (A).
Tightening torque 49.0 ~ 63.7 N.m (5.0 ~ 6.5 kgf.m, 36.2 ~ 47.0 lb-ft) 78.5 ~ 98.1 N.m (8.0 ~ 10.0 kgf.m, 57.9 ~ 72.3 lb-ft)

6. | Install in the reverse order of removal.

##### Sub Frame Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Loosen the bolt (A) and then disconnect the universal joint assembly from the pin ...

##### Rear Suspension System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage cable Repair procedures

Removal [High voltage battery pack - High voltage joint box] • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the front door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m,12.3 ~ 15.9 lb-ft) 2. Detach the clips, and then remove the front door side weatherstrip (A). 3. Install in the reverse order of removal. ...
Copyright © www.ksoulev.com 2020-2021