- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heat Pump / Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heat Pump / Description and Operation

Heat Pump Configuration and Operation

Heat pump is configured to circulate refrigerant flow for cooling/heating function.
This process minimizes battery consumption by the heater resulting in enhanced driving distance of EV.

[Heating]

1. | Outer Condenser - Evaporates liquid refrigerant and forms low temp-low pressure gas substance.

2. | 3-Way Solenoid Valve #2 - Redirects the refrigerant direction towards the chiller when heat pump is active.

3. | Chiller - Uses waste heat from the motor and performs secondary heat exchange on low temp-low pressure gas.

4. | Accumulator - Separates gas/liquid so that only the refrigerant in gas state can flow into the compressor.

5. | Electric Compressor - Compressor is operated by electric motor. Converts low temp-low pressure gas refrigerant into high temp-high pressure gas and sends it to inner condenser.

6. | Inner Condenser - Condenses high temp-high pressure gas refrigerant and transforms it into high temp-high pressure liquid refrigerant.

7. | 2-Way Solenoid Valve #1 - Instantly expands refrigerant to create low temp-low pressure refrigerant.

8. | 2-Way Solenoid Valve #2 - Sends the refrigerant to the evaporator if DEFROST Mode is used when heating.

9. | 3-Way Solenoid Valve #1 - Bypasses the refrigerant to chiller if refrigerant accumulation in the outer condenser is detected.

[Cooling]

1. | Outer Condenser - Condenses high temp-high pressure gas refrigerant and transforms it into high temp-high pressure liquid refrigerant.

2. | 3-Way Valve #2 - Directs refrigerant flow to expansion valve when A/C is operating.

3. | Expansion Valve - Instantly expands refrigerant to create low temp-low pressure gas.

4. | Evaporator - Operates blower fan to cool the air passing through the evaporator pin while the refrigerant in foggy state is transformed into gas (surrounding area gets cold).

5. | Accumulator - Separates gas/liquid so that only gas state refrigerant can flow into the compressor.

6. | Electric Compressor - Compressor is operated by electric motor. Converts low temp-low pressure gas refrigerant into high temp-high pressure gas and sends it to inner condenser.

7. | Inner Condenser - Condenses high temp-high pressure gas refrigerant and transforms it into high temp-high pressure liquid refrigerant.

8. | 2-Way Solenoid Valve #1 - Does not expand but circulates refrigerant when A/C is operating.

9. | 2-Way Solenoid Valve #2 - Prevents refrigerant from flowing into evaporator.

10. | 3-Way Solenoid Valve #1 - Circulates refrigerant to outer condenser.

##### Heat Pump

...

##### Refrigerant Direction Control Valve Components and Components Location

Components Location 1. 3-Way Solenoid Valve Assembly2. 2-Way Solenoid Valve Assembly ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. Front seat headrest2. Front seat headrest guide3. Front seat back cover4. Front seat back heater5. Front seat back pad6. Front seat back lumbar assembly7. Front seat back frame assembly8. Front seat back board9. Front seat cushion cover10. Front seat cushion heater11. Front seat c ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Latch Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021