- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Charging System / Normal Charge Cable Lock Actuator Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Charging System / Normal Charge Cable Lock Actuator Repair procedures

Removal and Installation

1. | Shut off the high voltage. (Refer to Battery Control System – “High Voltage Shut-off Procedure”)

2. | Disconnect the auxiliary battery (12V) negative (-) terminal.

3. | Disconnect the connector (A).

4. | Remove the actuator by loosening the bolts (B).
Tightening torque : 0.98-3.92 N.m (0.1-0.4 kgf.m, 0.72-2.9 lb-ft)

5. | Install in the reverse order of removal.

##### Normal Charge Cable Lock Actuator Description and Operation

Description and Operation It prevents the normal charge cable theft by operating the actuator when the door is locked.The normal charge cable can be connected only when the door is unlocked. An ...

##### High Voltage Distributing System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Glove Box Housing Components and Components Location

Component Location 1. Glove box housing ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: TPMS Sensor Description and Operation

Description Mode of Operation ASIC Mode 1. Factory Mode The factory mode is the mode that allows the TPM sensor to transmit RF Frames and sample LF more often in the HKMC factory. The TPM sensor will send normal RF frames in factory mode. LF sampling will occur every 1 second, to ensu ...
Copyright © www.ksoulev.com 2020-2021