- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Driveshaft and axle / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Driveshaft and axle / Specifications

Specification

Motor | Joint type | Max. permissible angle
Outer | Inner | Outer | Inner
80KW | BJ#92 | TJ#92 | 45° | 21°

Tightening Torques

Item | N.m | kgf.m | Ib.ft
Front | Tire wheel hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Drive shaft coking nut | 274.6 ~ 294.2 | 28.0 ~ 30.0 | 202.5 ~ 217.0
Strut assembly to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Caliper guide rod bolt | 21.6 ~ 31.4 | 2.2 ~ 3.2 | 15.9 ~ 23.1
Brake caliper mounting bolt | 78.4 ~ 98.0 | 8.0 ~ 10.0 | 57.8 ~ 72.3
Wheel speed sensor mounting bolt | 6.8 ~ 10.7 | 0.7 ~ 1.1 | 5.0 ~ 7.9
Brake disc mounting screw | 4.9 ~ 5.8 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Lower arm to knuckle | 58.8 ~ 70.6 | 6.0 ~ 7.2 | 43.4 ~ 52.1
Tie rod end ball joint nut | 23.5 ~ 33.3 | 2.4 ~ 3.4 | 17.4 ~ 24.5
Rear | Tire wheel hub nuts | 88.2 ~ 107.8 | 9.0 ~ 11.0 | 65.0 ~ 79.5
Rear caliper guide rod bolt | 21.6 ~ 31.4 | 2.2 ~ 3.2 | 15.9 ~ 23.1
Rear caliper to torsion beam axle | 63.7 ~ 73.5 | 6.5 ~ 7.5 | 47.0 ~ 54.2
Rear hub assembly to torsion beam axle | 49.0 ~ 58.8 | 5.0 ~ 6.0 | 36.2 ~ 43.3
Disc fixing screw | 4.9 ~ 5.9 | 0.5 ~ 0.6 | 3.6 ~ 4.3

Lubricants

Motor | Joint | Lubricants | Quantity
80KW | BJ | GRB006 | 105g (+10g/0)
TJ | SH06-VX21 | 140g (+10g/0)

##### High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage syst ...

##### Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionBand installer09495-3K000Used to install ear type boot bandPuller09495-33000Used to remove spider assemblyBall joint puller09568-340 ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Belt Outside Weatherstrip Repair procedures

Replacement 1. Pull down rear door window glass by pressing the power window glass switch. 2. After loosening the mounting screws, remove the rear door belt outside weatherstrip (A). 3. Install in the reverse order of removal. • Replace any damaged ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Wheel Guard Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...
Copyright © www.ksoulev.com 2020-2021