- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Glass Defogger / Rear Glass Defogger Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Rear Glass Defogger / Rear Glass Defogger Switch Repair procedures

Inspection

1. | The windshield deicer switch inputs can be checked using the GDS.

2. | To check the input value of windshield deicer switch, select "Body Control Module" menu.

3. | Select "Current Data" menu.

4. | To perform functional test on SJB outputs, select "Actuation Test".

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the heater and A/C control unit. (Refer to Heating, Ventilation, Air Condition - "Heater & A/C Control Unit (FATC))

Installation

1. | Install the heater and A/C control unit.

2. | Connect the negative (-) battery terminal.

##### Rear Glass Defogger Printed Heater Repair procedures

Inspection Wrap tin foil around the end of the voltmeter test lead to prevent damaging the heater line. Apply finger pressure on the tin foil, moving the tin foil a ...

##### Rear Wiper/Washer

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: General Information

Lift And Support Points When heavy rear components such as suspension, fuel tank, spare tire, tailgate and trunk lid are to be removed, place additional weight in the luggage area before hoisting. When substantial weight is removed from the rear of the vehicle, ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Information Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Using the flat screw driver or remover, remove the crash pad center air vent panel (A). 3. Disconnect the hazard switch connector (A). 4. Remove center fascia upper panel (A) after loosening the mounting screws. 5. Disco ...
Copyright © www.ksoulev.com 2020-2021