- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Charge Door Opener Cover / Charge Door Opener Actuator Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Charge Door Opener Cover / Charge Door Opener Actuator Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front bumper cover. (Refer to Body - "Front Bumper Cover")

3. | Remove the charge door opener cover assembly. (Refer to Body - "Charge Door Opener Cover")

4. | Remove the charge door opener actuator cable (A).

5. | Remove the charge door opener actuator (C) after loosening the mounting bolts (A) and screws (B).

Installation

1. | Install the charge door opener actuator and cable.

2. | Install the charge door opener cover assembly on the front bumper cover.

3. | Install the front bumper cover.

4. | Connect the negative (-) battery terminal.

Inspection

1. | Remove the connector from the charge door opener actuator.

2. | Connect battery positive (+) and negative (-) cables to terminals 1 and 2 respectively.

3. | Check that the motor operates normally. Replace the motor if it operates abnormally.

##### Components and Components Location

Components Location 1. Charge door opener actuator switch2. Charge door opener actuator3. Charge door opener cover ...

##### Charge Door Opener Actuator Switch Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cowl Side Trim Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Height Adjust Repair procedures

Replacement 1. Remove the front seat belt upper anchor. (Refer to Front Seat Belt - "Front Seat Belt Pretensioner") 2. After loosening the mounting bolts, remove the height adjust (A). Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5kgf.m, 28.9 ~ 39.8 lb-ft) 3. Install in the rever ...
Copyright © www.ksoulev.com 2020-2021