- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heating,Ventilation, Air Conditioning / Special Service Tools

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Special Service Tools

Special Service Tools

Personal Protective Equipment

Name | Illustration | Description
Insulation gloves |  | Used when inspecting or working on the high voltage components [Insulation performance : 1000V / 300A or above]
Insulation shoes |  | Used when inspecting or working on the high voltage components
Insulation clothes |
Insulation helmet |
Safety glasses |  | Used in the following cases : • When removing, installing or inspecting the high voltage battery terminals or wiring where spark may occur. • When working on the high voltage battery pack assembly.
Face shield |
Insulation mat |  | Removed high voltage components are placed on the insulation mat to prevent safety accidents.
Insulation sheet |  | High voltage components are covered with insulation sheet to protect people not wearing personal protective equipment from safety accidents.

##### Specifications

Specification Air Conditioner ItemSpecificationCompressorTypeESC33n (Electric Scroll)Communication typeCAN communicationOil type & CapacityPOE OIL, 180±10gMotor typeBLDCRated voltage360VOpe ...

##### Troubleshooting

Troubleshooting Problem Symptoms Table Before replacing or repairing air conditioning components, first determine if the malfunction is due to lack of refrigerant, air flow or compressor. U ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Auto Light Sensor Repair procedures

Inspection In the state of IGN1 ON, when the multi function switch module detects auto light switch on, tail lamp relay output and head lamp low relay output are controlled according to auto light sensor''s input. During IGN1 ON, the BCM monitors the range of this supply and alerts the f ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Panorama Sunroof Switch Repair procedures

Inspection 1. Disconnect the negative (-) battery terminal. 2. Open the sunglass case cover from the overhead console then remove the 2 screws holding the overhead console. Disconnect the switch connector and Map lamp connector, and then remove the overhead console lamp (A). 3. Che ...
Copyright © www.ksoulev.com 2020-2021