- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Repair procedures

Adjustment

Glass Adjustment

• | Check the glass run channels for damage or deterioration, and replace them if necessary.

1. | Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim")

2. | Remove the rear door window glass mounting hole plug (A).

3. | Carefully move the rear door window glass (A) until the glass mounting bolt are visible, then loosen them.

4. | Check that the glass moves smoothly.

Door Striker Adjustment

• | Make sure that the door latches securely without slamming it. If necessary, adjust the striker (A) by moving it up and down or in and out before fixing the striker nuts.

1. | Loosen the screws (B) just enough for the striker to move.
Tightening torque : (B) : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m, 12.3 ~ 15.9 lb-ft)

2. | Lightly tap on the striker with a plastic hammer just enough to give some adjustment.

3. | Hold the outer handle out, and push the door against the body to be sure the striker allows a flush fit. If the door latches properly, tighten the screws and recheck.

Door Position Adjustment

• | After installing the door, check for a flush fit with the adjacent body panels, then check for equal gaps between the front, rear, and bottom, door edges and the body. Check that the door and body edges are parallel. Before adjusting, replace the mounting bolts.

1. | Check that the door and body edges are parallel.

2. | Place the vehicle on a firm, level surface when adjusting the doors.

3. | Adjust at the hinges (A):
• | Loosen the door mounting bolts slightly, and move the door in or out until it aligns flush with the body.
• | Loosen the hinge mounting bolts slightly, and move the door backward or forward, up or down as necessary to equalize the gaps.
• | Place a shop towel on the jack to prevent damage to the door when adjusting the door.
Tightening torque : (B) : 21.6 ~ 26.5 N.m (2.2 ~ 2.7 kgf.m, 15.9 ~ 19.5 lb-ft) (C) : 34.2 ~ 41.2 N.m (3.5 ~ 4.2 kgf.m, 25.3 ~ 30.4 lb-ft)

4. | Grease the pivot portions of the hinges as indicated by the arrows.

5. | Check for water leakage.

##### Components and Components Location

Components (1) 1. Rear door pull cap2. Rear door inside handle cap3. Rear door delta inner cover4. Rear door trim5. Rear door belt inside weatherstrip6. Rear door panel7. Rear door delta garnish ...

##### Rear Door Trim Components and Components Location

Component Location 1. Rear door trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cluster ionizer Description and Operation

Description The cluster ionizer makes disinfection and decomposition of bad smell from the air-conditioner or inflow air. And it cleans the inside air of a vehicle. When the air-conditioner or heater is operating, it starts from "CLEAN" mode and alternates from "CLEAN" mode to "ION" mode a ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Inspection

Inspection When removing the battery pack assembly to inspect the battery system, it can be connected to vehicle by using the SST 0K918-E4100, 0K375-E4100, 0K375-E4200. Before installing the battery system assembly, check if the battery is OK by using the SST. ...
Copyright © www.ksoulev.com 2020-2021