- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tires/Wheels / Wheel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Tires/Wheels / Wheel Repair procedures

Hub nut tightening sequence

Tighten the hub nuts as follows.

Tightening torque: 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)

When using an impact gun, final tightening torque should be checked using a torque wrench.

Run out inspection

1. | Jack up the vehicle.

2. | Measure the wheel Run-out by using a dial indicator as illustration below.
Run-out | Aluminum
Radial mm(in.) | Below 0.3(0.0118)
Lateral mm(in.) | Below 0.3(0.0118)

3. | If measured value exceeds the standard value, replace the wheel.

##### Tire Repair procedures

Tire Wear 1. Measure the tread depth of the tires. Tread depth [limit] : 1.6 mm (0.0630 in.) 2. If the remaining tread depth (A) is less than the limit, replace the tire. &nb ...

##### Alignment Repair procedures

Front wheel alignment When using a commercially available computerized wheel alignment equipment to inspect the front wheel alignment, always position the vehicle o ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification MotorJoint typeMax. permissible angleOuterInnerOuterInner80KWBJ#92TJ#9245°21° Tightening Torques ItemN.mkgf.mIb.ftFrontTire wheel hub nuts88.3 ~ 107.99.0 ~ 11.065.1 ~ 79.6Drive shaft coking nut274.6 ~ 294.228.0 ~ 30.0202.5 ~ 217.0Strut assembly to knuckle137.3 ~ 156.914.0 ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Repair procedures

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be su ...
Copyright © www.ksoulev.com 2020-2021