- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Hood / Hood Latch Release Handle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Hood / Hood Latch Release Handle Repair procedures

Replacement

1. | Using a screwdriver or remover, remove the hood release handle (A).
• | Use a 6mm hex bit to press the center until the handle easily pulls off the post.

2. | Install in the reverse order of removal.
• | Make sure that the hood latch cable is connected properly.
• | Make sure that the hood locks/unlocks and opens/closes properly.

##### Hood Latch Release Handle Components and Components Location

Component Location 1. Hood latch release handle ...

##### Hood Latch Components and Components Location

Component Location 1. Hood lower latch assembly ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Luggage Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Using a screwdriver or remover, remove the luggage lamp (A). 3. Remove the luggage lamp (A) after disconnecting the connector (B). Installation 1. Install the luggage lamp assembly after connecting the lamp connector. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Temperature Sensor Repair procedures

Inspection High voltage battery heater temperature sensor is installed in modules No. 1 and No. 8. 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure") 3. Remove the high volt ...
Copyright © www.ksoulev.com 2020-2021