- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Cooling System / Inlet Temperature Sensor Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Cooling System / Inlet Temperature Sensor Specifications

Specification

Temperature (°C) | Resistance (K?) | Tolerance (%)
-40 | 204.5 | ±4.0
-30 | 117.8 | ±3.5
- 20 | 70.34 | ±3.0
- 10 | 43.43 | ±2.5
0 | 27.63 | ±2.0
10 | 18.07 | ±1.6
20 | 12.11 | ±1.2
30 | 8.303 | ±1.2
40 | 5.813 | ±1.5
50 | 4.149 | ±1.9
60 | 3.013 | ±2.2
70 | 2.225 | ±2.5

##### Cooling Duct Repair procedures

Removal Battery Module Outlet Duct • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the hi ...

##### Inlet Temperature Sensor Description and Operation

Description Inlet temperature sensor is installed on the No.8 module of high voltage battery and it detects the inner air temperature of battery. The operation of cooling fan depends on the inl ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: PWM Blower Module Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Manually operate the control switch and measure the voltage of blower motor. 3. Select the control switch to raise voltage until high speed. Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove the glove box housin ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Console Cover Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021