- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body (Interior and Exterior) / Front Seat

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Seat

- Components and Components Location
- Front Seat Assembly Components and Components Location
- Front Seat Assembly Repair procedures
- Front Seat Shield Outer Cover Components and Components Location
- Front Seat Shield Outer Cover Repair procedures
- Front Seat Shield Inner Cover Components and Components Location
- Front Seat Shield Inner Cover Repair procedures
- Front Seat Back Cover Components and Components Location
- Front Seat Back Cover Repair procedures
- Front Seat Cushion Cover Components and Components Location
- Front Seat Cushion Cover Repair procedures
- Front Seat Frame Assembly Components and Components Location
- Front Seat Frame Assembly Repair procedures

##### Front Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the front door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m,12.3 ~ 15.9 lb-ft) 2. Detach the clips, and then remove the front doo ...

##### Components and Components Location

Components 1. Front seat headrest2. Front seat headrest guide3. Front seat back cover4. Front seat back heater5. Front seat back pad6. Front seat back lumbar assembly7. Front seat back frame asse ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Temperature Sensor Repair procedures

Inspection High voltage battery heater temperature sensor is installed in modules No. 1 and No. 8. 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure") 3. Remove the high volt ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification ItemSpecificationRated voltageDC 3VOperating voltageDC 2.7V ~ 3.3VOperating temperature-20°C ~ +60°C (-4°F ~ +140°F)RF ModulationFSKLF ModulationASKRF frequency433.92 MHzBatteryCR2032 (3V / 1EA)Transmissible distance30m or moreBattery lifetime2 years or more (at 20 times per d ...
Copyright © www.ksoulev.com 2020-2021