- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Crash Pad Lower Panel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Crash Pad Lower Panel Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the cowl side trim. (Refer to Interior Trim - "Cowl Side Trim")

2. | Using a screwdriver or remover, remove the crash pad side cover [LH] (A).

3. | After loosening the mounting screws, remove the crash pad lower panel (A) using a screw driver.

4. | Disconnect the diagnosis connector (A).

5. | Install in the reverse order of removal.
• | Make sure that the connectors are connected properly.
• | Replace any damaged clips.

##### Crash Pad Lower Panel Components and Components Location

Component Location 1. Crash pad lower panel ...

##### Glove Box Housing Components and Components Location

Component Location 1. Glove box housing ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Components and Components Location

Component 1. Battery Heater2. Battery Heater Relay3. Battery Heater Fuse4. Battery Heater Temperature Sensor ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Roller Blind Repair procedures

Removal 1. Open the roller blind using the panorama sunroof switch. • Leave 10 ~ 20cm (0.3937 ~ 0.7874 in) of the roller blind unopened. 2. Remove the roof trim. (Refer to Roof Trim - "Roof Trim Assembly") 3. Remove the roller blind bar (C) by ...
Copyright © www.ksoulev.com 2020-2021