- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Parking Assist System / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Parking Assist System / Specifications

Specifications

Item | Specification
Front/Rear parking assist system control unit | Rated voltage | DC 12V
Operation range | 30~120 cm(11.8~47.2 in)
Operation voltage | DC 9V~16V
Operation current | Max. 300 mA
Operation temperature | -30~+80 °C
Operation frequency | 48 ± 5 KHz
Number of sensors | Front : 4EA(Left, Right, Center left, Center right) Rear : 4EA(Left, Right, Center left, Center right)

##### Parking Assist System

...

##### Components and Components Location

Component Location 1. BCM2. Ultrasonic sensor ? Parking assist control unit function and buzzer are built in BCM (body control unit). ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Driver Airbag (DAB) Module and Clock Spring Description and Operation

Description Driver Airbag (DAB) is installed inside the steering wheel and is electrically connected to SRSCM with a clock spring. It protects the driver from impact by deploying a bag when frontal crash occurs. The SRSCM determines the deployment of Driver Airbag (DAB). ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Wheel Repair procedures

Hub nut tightening sequence Tighten the hub nuts as follows. Tightening torque: 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft) When using an impact gun, final tightening torque should be checked using a torque wrench. Run out inspection 1. Jack up the ...
Copyright © www.ksoulev.com 2020-2021