- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Multifunction Switch / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Multifunction Switch / Specifications

Specifications

Items | Specifications
Rated voltage | DC 12V
Operating temperature range | -30°C ~ +80°C (-22 ~ +176°F)
Rated load | Dimmer & passing switch | High : 1A (Relay load)
Low : 1A (Relay load)
Passing : 1A (Relay load)
Lighting switch/ Auto lighting switch | 1A (Relay load)
Turn signal & lane change switch | 6.6 ± 0.5A (Lamp load)
Front / Rear fog lamp switch | 1A (Relay load)
Wiper switch | Low, High : 4.0A (Motor load)
Intermittent : 0.22 ± 0.05A (Relay load)
Lock : Max. 28A (Motor load)
Mist switch | Mist : 4A (Motor load)
Front/Rear washer switch | 4A (Motor load)
Rear wiper | 0.2A (Relay load)

##### Multifunction Switch

...

##### Components and Components Location

Component ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description System Overview The System offers the following features: – Human machine interface through a 1-stage button, for terminal switching and engine start. – Control of external relays for ACC / IGN1 / IGN2 terminal switching and STARTER, without use of mechanical i ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Seat Heater Switch Schematic Diagrams

Circuit Diagram [First Row Seat] Second Row Seat ...
Copyright © www.ksoulev.com 2020-2021