- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Air Conditioning System / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Air Conditioning System / Repair procedures

Refrigerant System Service Basics

• | Since the electric compressor uses high-voltage, POE oil with high volumetric resistivity should be used.

• | Do not use the same A/C recovery / charging station as in conventional belt-driven compressors.

• | If PAG oil mixes into the POE oil of the system, dielectric breakdown may occur due to decreased volumetric resistivity and the A/C compressor may not work.

Refrigerant Recovery
Use only U.L.-listed service equipment that is certified to meet the requirements of SAE J2210 when removing HFC-134a (R-134a) from the air conditioning system.

• | Air conditioning refrigerant or lubricant vapor can irritate your eyes, nose, or throat.
• | Be careful when connecting service equipment.
• | Do not breathe refrigerant or vapor.

If accidental system discharge occurs, ventilate work area before resuming to service.
Additional health and safety information may be obtained from the refrigerant and lubricant manufacturers.

1. | Connect an R-134a refrigerant Recovery/Recycling/Charging System (A) to the high-pressure service port (B) and the low-pressure service port (C) as shown, following the equipment manufacturer''s instructions. [Without Heat Pump] [With Heat Pump]

2. | Measure the amount of refrigerant oil removed from the A/C system after the recovery process is completed. Be sure to install the same amount of new refrigerant oil back into the A/C system before charging.

System Evacuation
Use only U.L.-listed service equipment that is certified to meet the requirements of SAE J2210 when removing HFC-134a (R-134a) from the air conditioning system.

• | Air conditioning refrigerant or lubricant vapor can irritate your eyes, nose, or throat.
• | Be careful when connecting service equipment.
• | Do not breathe refrigerant or vapor.

If accidental system discharge occurs, ventilate work area before resuming to service.
Additional health and safety information may be obtained from the refrigerant and lubricant manufacturers.

1. | When an A/C System has been opened to the atmosphere, such as during installation or repair, it must be evacuated using an R-134a refrigerant Recovery/Recycling/Charging System. (If the system has been open for several days, the receiver/dryer should be replaced, and the system should be evacuated for several hours.)

2. | Connect an R-134a refrigerant Recovery/Recycling/Charging System (A) to the high-pressure service port (B) and the low-pressure service port (C) as shown, following the equipment manufacturer''s instructions.

3. | If the pressure does not reach over 93.3 kPa (700 mmHg, 27.6 in.Hg) in 10 minutes, there may be a leakage in the system. Partially charge the system and check for any leakages (see Leak Test).

4. | Remove the low pressure valve from the low-pressure service port.

System Charging
Use only U.L.-listed service equipment that is certified to meet the requirements of SAE J2210 when removing HFC-134a (R-134a) from the air conditioning system.

• | Air conditioning refrigerant or lubricant vapor can irritate your eyes, nose, or throat.
• | Be careful when connecting service equipment.
• | Do not breathe refrigerant or vapor.

If accidental system discharge occurs, ventilate work area before resuming to service.
Additional health and safety information may be obtained from the refrigerant and lubricant manufacturers.

1. | Connect an R-134a refrigerant Recovery/Recycling/Charging System (A) to the high-pressure service port (B) as shown, following the equipment manufacturer''s instructions.

2. | Add the same amount of new refrigerant oil to system that was removed during recovery. Use only specified refrigerant oil. Charge the system with R-134a refrigerant. Do not overcharge the system as it may damage the compressor.
Specified amount Without heat pump : 550 ± 25g (19.4 ± 0.88 oz.) With heat pump : 900 ± 25g (31.7 ± 0.88 oz.)

Refrigerant Leak Test
Always conduct a leak test with an electronic leak detector whenever leakage of refrigerant is suspected and when conducting service operations that accompany disassembling, loosening or connecting of fittings.

• | In order to use the leak detector properly, read the manual supplied by the manufacturer.

If a gas leak is detected, proceed as follows:

1. | Check the tightening torque of the connection fittings, and if it is too loose, tighten to the proper torque. Using a leak detector (A), check for gas leakage.

2. | If leakage continues even after the fitting has been tightened, discharge the refrigerant from the system, disconnect the fittings, and check their seating faces for damage. Replace at all times even for a slight damage.

3. | Check the compressor oil and add oil if required.

4. | Charge the system and recheck for gas leaks. If no leaks are found, evacuate and charge the system again.

##### Description and Operation

Refrigeration Cycle ...

##### Components and Components Location

Component Location Index Engine Room [Without Heat Pump] 1. Receiver-drier2. Condensor3. A/C Pressure Transducer (APT)4. Service port (Low pressure)5. Service port (High pressure)6. Sucti ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Assembly Components and Components Location

Component Location 1. Tail gate assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Latch Components and Components Location

Component Location 1. Tail gate latch assembly ...
Copyright © www.ksoulev.com 2020-2021