- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: AVN System / Audio Remote Control Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / AVN System / Audio Remote Control Repair procedures

Inspection

1. | Check for resistance or output voltage between terminals in each switch position. [Audio]
Switch | Connector terminal | Resistance (±5%) | Output voltage
Seek up | 2-4 | 430 ? | 0.4 V ± 0.22
Seek down | 2-4 | 1.1 k? | 1.0 V ± 0.22
Mode | 2-4 | 2.11 k? | 1.5 V ± 0.22
Mute | 2-4 | 3.11 k? | 2.0 V ± 0.22
Volume up | 2-4 | 4.61 k? | 2.5 V ± 0.22
Volume down | 2-4 | 6.81 k? | 3.0 V ± 0.22
[Cruise]
Switch | Connector terminal | Resistance (±5%) | Output voltage
Cancel | 2-4 | 180 ? | 0.8 V ± 0.17
Set | 2-4 | 330 ? | 1.2 V ± 0.17
Resume | 2-4 | 550 ? | 1.8 V ± 0.22
Cruise | 2-4 | 880 ? | 2.3 V ± 0.22
Speed limit | 2-4 | 2.54 k? | 3.6 V ± 0.22
[Voice + Bluetooth]
Switch | Connector terminal | Resistance (±5%) | Output voltage
Voice | 2-4 | 10.71 k? | 3.5 V ± 0.22
Call off | 2-4 | 18.91 k? | 4.0 V ± 0.22
Call | 2-4 | 40.91 k? | 4.5 V ± 0.22
[Flex steer + Trip + Reset]
Switch | Connector terminal | Resistance (±5%) | Output voltage
Flex steer | 2-4 | 180 ? | 0.8 V ± 0.17
Trip | 2-4 | 330 ? | 1.2 V ± 0.17
Reset | 2-4 | 550 ? | 1.8 V ± 0.22

Removal

[Upper Steering Wheel Remote Control Switch]

1. | Disconnect the negative (-) battery terminal.

2. | Remove the driver airbag module. (Refer to the RT group)

3. | Remove the steering wheel. (Refer to the ST group - "Steering column & shaft")

4. | Loosen the mounting screws from the rear steering wheel cover.

5. | Separate the upper steering wheel remote control switch (A) from the steering wheel. [LH] [RH]

6. | Remove the upper steering wheel control switch (B) disconnecting the connector (A). [LH] [RH]

[Lower Steering Wheel Remote Control Switch]

1. | Disconnect the negative (-) battery terminal.

2. | Remove the driver airbag module. (Refer to the RT group)

3. | Remove the steering wheel. (Refer to the ST group - "Steering column & shaft")

4. | Loosen the mounting screws from the rear steering wheel cover.

5. | Separate the upper steering wheel remote control switch (A) from the steering wheel. [LH] [RH]

6. | Remove the upper steering wheel control switch (B) disconnecting the connector (A). [LH] [RH]

7. | Separate the lower steering wheel control switch (A) loosening the mounting screws. [LH] [RH]

8. | Remove the lower steering wheel control switch (B) disconnecting the connector (A). [LH] [RH]

Installation

1. | Install the remote control switch on the steering wheel.

2. | Install the steering wheel.

3. | Reconnect the remote control switch connector and airbag connectors.
Make sure that the switch connector is plugged in properly.

4. | Install the driver airbag module.

5. | Connect the negative (-) battery terminal.

##### Audio Remote Control Schematic Diagrams

Circuit Diagram ...

##### Multimedia Jack Schematic Diagrams

Circuit Diagram ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Inspection

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be su ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Adjustment 1. After loosening the tail gate hinge (A) mounting bolt, adjust the tail gate by moving it up and down, or right and left. 2. Adjust the tail gate height by turning the tail gate overslam bumpers (B). 3. After loosening the tail gate striker (C) mounting bolts, adjust the t ...
Copyright © www.ksoulev.com 2020-2021