- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Seat Electrical / Seat Heater Switch Components and Components Location

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Seat Electrical / Seat Heater Switch Components and Components Location

Components

[First Row Seat]

Connector Pin Information

Pin No. | Connector A | Connector B | Connector C
1 | Illumination (+) | Ground | Electric compressor - interlock (+)
2 | Sensor REF (+5V) | Sensor ground | Electric compressor - interlock (-)
3 | C_CAN High | PWM blower IN | High voltage PTC heater - interlock (+)
4 | C_CAN LOW | Cluster ionizer diagnosis | High voltage PTC heater - interlcok (-)
5 | Driver mode actuator (VENT) | - | PAB IGN3
6 | Driver mode actuator (DEF) | CLEAN signal | PAB ON signal
7 | Driver mode actuator F/B | Assist mode actuator (VENT) | PAB OFF signal
8 | Intake actuator (FRE) | Assist mode actuator (DEF) | SBR
9 | Intake actuator (REC) | Assist mode actuator F/B | Rr LEFT SBR
10 | Extake actuator F/B | DEF actuator (OPEN) | Rr CENTER SBR
11 | K-LINE | DEF actuator (CLOSE) | Rr RIGHT SBR
12 | HTD | DEF actuator F/B | -
13 | Rear defog switch | Vent left duct sensor (+) | -
14 | Temperature control actuator (COOL) | Floor left duct sensor (+) | -
15 | Temperature control actuator (WARM) | IGN3 | -
16 | Temperature control actuator F/B | IGN2 | -
17 | Driver seat heater indicator - LOW | - |
18 | Driver seat heater indicator - MID | 2 WAY valve #1 (+)
19 | Driver seat heater indicator - HIGH | 3 WAY valve #1 (+)
20 | Illumination (RHEO) | 3 WAY valve #2 (+)
21 | DETENT OUT (+) | 2 WAY valve #2 (+)
22 | Driver seat heater switch | CLIMATE_CAN HIGH
23 | Driver cooler seat indicator - LOW | CLIMATE_CAN LOW
24 | Driver cooler seat indicator - MID | HUMIDITY (PWM)
25 | Driver cooler seat indicator - HIGH | Air pressor tranduser signal
26 | Assist seat heater switch | Refrigerant temperature sensor signal #1
27 | Ambient sensor (+) | Refrigerant temperature sensor signal #2
28 | EVAP sensor (+) | Coolant 3way valve output
29 | Assist cooler seat indicator - LOW | IGN3
30 | Assist cooler seat indicator - MID | Blower IS
31 | Assist cooler seat indicator - HIGH | Battery
32 | Photo sensor (-) | Battery |
33 | Assist cooler switch | ?
34 | Driver cooler switch
35 | Blower INH
36 | MM_CAN HIGH
37 | MM_CAN LOW
38 | Assist seat heater indicator - LOW
39 | Assist seat heater indicator - MID
40 | Assist seat heater indicator - HIGH

Second Row Seat

##### Seat Electrical

...

##### Seat Heater Switch Schematic Diagrams

Circuit Diagram [First Row Seat] Second Row Seat ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Wiper Motor Repair procedures

Inspection Rear Wiper Motor 1. Remove the connector from the rear wiper motor. 2. Connect battery positive (+) and negative (-) cables to terminals 2 and 1 respectively. 3. Check that the motor operates normally. Replace the motor if it operates abnormally. No.Description1Battery (+) ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Center Fascia Panel Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021