- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: AHB(Active Hydraulic Boost) System / Brake Actuation Unit Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / AHB(Active Hydraulic Boost) System / Brake Actuation Unit Repair procedures

Removal

1. | Turn ignition switch OFF and disconnect the negative (-) battery cable.

2. | Disconnect the brake fluid level switch connector (A), and remove the reservoir cap.
Be sure to completely remove foreign substances around brake fluid reservoir and cap before opening the reservoir cap to prevent any contamination of brake fluid and deterioration in braking performance.

3. | Using a syringe, remove the brake fluid from the reservoir.
• | Do not spill brake fluid on the vehicle as it may damage the paint. If brake fluid comes in contact with the paint, wash off immediately with water.
• | To prevent dust entering the reservoir, the reservoir cap should be closed again after removing brake fluid.

4. | Disconnect reservoir hose from the reservoir and IBAU connecter (A).

5. | Disconnect the brake tube from the IBAU by loosening the tube flare nut (B).
Before removing the IBAU, high pressure in an accumulator of PSU should be reduced for safety by conducting "High pressure release mode" of GDS connected to SOUL EV.
Tightening torque: 13.7 ~ 16.7 N.m (1.4 ~ 1.7 kgf.m, 10.1 ~ 12.3 lb-ft)

6. | Remove the brake pedal assembly. (Refer to the brake system group - brake pedal)

7. | Remove the IBAU mounting nuts (A) and then remove the IBAU.
Tightening torque: 12.7 ~ 15.7 N.m (1.3 ~ 1.6 kgf.m, 9.4 ~ 11.6 lb-ft)

Installation

1. | Install in the reverse order of removal.

2. | Check the brake pedal operation.

3. | After filling the brake fluid in the reservoir, perform the air bleed. (Refer to the AHB system - AHB system air bleeding)

4. | Conduct calibration after removing the brake pedal assembly. (Refer to the brake pedal - calibration)

##### Brake Actuation Unit Components and Components Location

Components IBAU must not be disassembled. 1. ECU2. Reservoir3. Master cylinder Assembly4. Valve block ...

##### Pressure Source Unit Components and Components Location

Components PSU must not be disassembled. 1. Motor connector2. Bracket3. Block4. Accumulator5. Damper6. Motor ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Back view camera2. AVN head unit ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Lift Repair procedures

Replacement • When removing and installing the hood lifter, work in a group of two or more. • When removing the clips, use a clip remover. 1. Using a screwdriver (A), lift the socket clips (B) up slightly on both ends of the lifter (D), a ...
Copyright © www.ksoulev.com 2020-2021