- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tire Pressure Monitoring System / Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Tire Pressure Monitoring System / Description and Operation

Description

TREAD Lamp

– | Tire Under Inflation / Leak Warning.

1. | Turn on condition
• | When tire pressure is below allowed threshold
• | When rapid leak is detected by the sensor.
• | Indicates that tire needs to be re-inflated to placard pressure / repaired.

2. | Turn off condition
• | Under-inflation ; When tire pressure is above (warning threshold + hysteresis).
• | Rapid Leak ; When tire pressure is above (leak warning threshold).

DTC Warning

1. | Turn on condition
• | When the system detects a fault that is external to the receiver/ sensor.
• | When the system detects a receiver fault.
• | When the system detects a sensor fault.

2. | Turn off condition
• | If the fault is considered as ''critical'', then the lamp is held on throughout the current Ignition cycle (even if the DTC has been demoted). This is because it is important to bring the problem to the drivers attention. On the following Ignition cycle, the demotion conditions will be re-checked. If the demotion conditions occur, the lamp will be turned off. It will be held on until DTC demotion checking is completed.
• | ''Non critical'' faults are those that can occur temporarily e.g. vehicle battery under voltage. The lamp is therefore turned off when the DTC demotion condition occurs.

• | When driving in high altitude grades, it is natural for the atmospheric pressure to decrease. Therfore, please check the tire pressure and add more air as necessary.
• | Tire pressure can be decreased naturally due to decrease in ambient temperature (especially in winter). In this case, fill tires with air to the specification if warning lamp is illuminated as this is natural phenomenon.

System Fault

1. | General Function
• | The system monitors a number of inputs across time in order to determine that a fault exists.
• | Faults are prioritized according to which has the most likely cause.
• | Certain faults are not covered through DTC. The main ones are:
a. | Sensor thermal shutdown (over 257°F/125°C).
b. | Ignition Line stuck ; requires observation of lamps at Ignition ON to diagnose.

##### Schematic Diagrams

Circuit Diagram Hamess Connector Pin No.Description1BATT+2IG_ON3CAN_L4CAN_H5NC6GND ...

##### Troubleshooting

TPMS Inspection method Inspection Find the inspection number by referring to the table above. The following content is irrelevant of the inspection procedure. 1. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Latch Components and Components Location

Component Location 1. Rear seat latch assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Replacement • Be careful not to damage the fender and body. • When removing the clips, use a clip remover. 1. Remove the head lamps. (Refer to Body Electrical System - "Head Lamps") 2. Remove the A pilla ...
Copyright © www.ksoulev.com 2020-2021