- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Door Locks / Power Door Lock Actuators Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Power Door Locks / Power Door Lock Actuators Repair procedures

Inspection

Front Door Lock Module Inspection

1. | Remove the front door trim. (Refer to Body - "Front Door Trim")

2. | Remove the front door module. (Refer to Body - "Front Door Module")

3. | Disconnect the connectors from the actuator.

4. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily. [Central Lock]

5. | Check for continuity between the terminals in each switch position according to the table.

Rear Door Lock Module Inspection

1. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

2. | Remove the rear door module. (Refer to Body - "Rear Door Module")

3. | Disconnect the connectors from the actuator.

4. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily. [Central Lock]

5. | Check for continuity between the terminals in each switch position according to the table.

Tailgate Lock Module Inspection

1. | Remove the tailgate trim. (Refer to Body - "Tailgate Trim")

2. | Disconnect the 4P connector from the actuator.

3. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

Tailgate Open Switch

1. | Remove the tailgate trim. (Refer to Body - "Tailgate Trim")

2. | Disconnect the connector from the actuator.

3. | Check for continuity between the terminals in each switch position according to the table.

Hood Switch

1. | Disconnect the connector (A) and bolts from the hood switch.

2. | Check for continuity between the terminals and ground according to the table.

##### Components and Components Location

Component Location 1. Driver power window main switch2. BCM (Body Control Module)3. Door lock switch4. Front door lock actuator & switch5. Rear door lock actuator & switch6. Tailgate lock ...

##### Power Door Lock Switch Repair procedures

Diagnosis With GDS 1. The BCM can be diagnosed by using the GDS. The BCM communicates with the GDS which then displays inputs and outputs along with codes. It will be able to quickly diagnose ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionHog ring clip installer09880-4F000Used to install hog ring clip Personal Protective Equipment NameIllustrationDescriptionInsulation glovesUsed when inspecting or working on the high voltage components[Insulation performance : ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Troubleshooting

Basic Troubleshooting Basic Inspection Procedure Measuring Condition of Electronic Parts'' Resistance The measured resistance at high temperature after vehicle running may be high or low. So all resistance must be measured at ambient temperature (20°C, 68°F), unless stated otherwise. ...
Copyright © www.ksoulev.com 2020-2021