- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Hood / Hood Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Hood / Hood Assembly Repair procedures

Replacement

• | Be careful not to damage the hood and body.

• | When removing and installing the hood, work in a group of two or more.
• | When removing the clips, use a clip remover.

1. | Using a screwdriver, lift the socket clips (A) up slightly on both ends of the lifter (B).

2. | After loosening the hood hinge (B) mounting bolts, remove the hood assembly (A).
Tightening torque : 21.6~26.5 N.m (2.2~2.7 kgf.m, 15.9~19.5 lb-ft)

3. | Install in the reverse order of removal.
• | Make sure that the hood locks/unlocks and opens/closes properly.
• | Adjust the hood alignment.

##### Hood Assembly Components and Components Location

Component Location 1. Hood assembly ...

##### Hood Lift Repair procedures

Replacement • When removing and installing the hood lifter, work in a group of two or more. • When removing the clips, use a clip remover. 1. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Door Opener Actuator Switch Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel") 3. Remove the crash pad lower switch assembly (A) by pushing it. 4. Disconnect the connector (A) from the crash pad lower switch assembly. 5. R ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Frame Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021