- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Charge Door Opener Cover / Charge Door Opener Actuator Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Charge Door Opener Cover / Charge Door Opener Actuator Switch Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel")

3. | Remove the crash pad lower switch assembly (A) by pushing it.

4. | Disconnect the connector (A) from the crash pad lower switch assembly.

5. | Remove the crash pad lower switch (A).

6. | If it is necessary to check the switch, check for continuity and measure the resistance between terminals.

Installation

1. | Install the crash pad lower switch.

2. | Install the crash pad lower panel after connecting the connector.

3. | Connect the negative (-) battery terminal.

##### Charge Door Opener Actuator Switch Components and Components Location

Components ...

##### Electro Chromic Inside Rear View Mirror

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Door Outside Handle Components and Components Location

Component Location 1. Front door outside handle ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Electric A/C compressor Specifications

Specification ModelESC33nMotorBLDC MotorControl TypeCANCompression TypeScrollCapacity33cc/revOperating Voltage Range190~320VRated Voltage288VMount TypeBracket Mounting, 4 Point Mounting ...
Copyright © www.ksoulev.com 2020-2021