- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Seat Electrical / Seat Heater (Air Ventilation) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Seat Electrical / Seat Heater (Air Ventilation) Repair procedures

Inspection

Front Seat

1. | Check for continuity and measure the resistance between terminals.
Part | Connector | Resistance (± 10%)
Cushion (C) | 1-4 | 4.54 ?
Back (B) | 1-4 | 5.16 ?
Set (A) | 3-4 | 9.70 ?
Performance of heater is the average temperature of seat surface. The temperatures of seat surface according to number of pushes on the seat heater switch are as follows.
Part | Type | 1st | 2nd | 3rd
First row seat | Cushion (±2°C/±35.6°F) | 3 Step | 36°C (96.8°F) | 39°C (102.2°F) | 42°C (107.6°F)
Back (±2°C/±35.6°F) | 40°C (104°F) | 45°C (113°F) | 50°C (122°F)

##### Seat Heater (Air Ventilation) Schematic Diagrams

Circuit Diagram ...

##### Air Ventilation Seat Control Unit Components and Components Location

Component Location 1. Seat back blower2. Seat cushion blower3. Air ventilation seat control unit ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Fender Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components Location 1. Torsion beam axle2. Shock absorber3. Coil spring assembly ...
Copyright © www.ksoulev.com 2020-2021