- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Pre-charge Relay Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Pre-charge Relay Repair procedures

Inspection

• | Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries.
• | Be sure to shut off the high voltage before doing any work related with the high voltage system(Refer to "High Voltage Shut-off Procedure"). Failure to follow the safety instructions may result in serious electrical injuries.

When removing the battery pack assembly to inspect the battery system, it can be connected to vehicle by using the SST 0K918-E4100, 0K375-E4100, 0K375-E4200. Before installing the battery system assembly, check if the battery is OK by using the SST.

Pre Charge Relay Inspection

[Using multi tester (Relay OFF)]

Inspect the high voltage pre-charge relay by using multi tester when the relay is off

1. | Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure")

2. | Remove the high voltage battery upper case. (Refer to High Voltage Battery System - "Case")

3. | Measure the resistance between the high voltage (+) power terminal and the joint box (+) terminal.
Specification : ??(20°C)

[Using GDS (Relay ON)]

1. | Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure")

2. | Remove the high voltage battery upper case. (Refer to High Voltage Battery System - "Case")

3. | Connect the SST(0K918-E4100, 0K375-E4100, 0K375-E4200) to the vehicle.

4. | Connect the GDS to DLC.

5. | Turn the ignition swtich ON.

6. | Activate the pre charge relay by using "Actuation Test" on the GDS as shown in the illustration below.
When the relay is ON, there is a relay operation sound.

Pre Charge Relay Coil Resistance

1. | Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure")

2. | Remove the power relay assembly (PRA) (Refer to High Voltage Battery System - "Power Relay Assembly (PRA)")

3. | Measure the resistance between pins No. 6 and No. 8 of the power relay assembly connector.
Specification : 104.4 ~ 127.6 ? (20°C)

Removal

Main Relay, Pre Charge Relay, Pre Charge Resistor, Battery Current Sensor, High Voltage Battery Heater Relay and the High Voltage Battery Heater Fuse are integrated in the Power Relay Assembly (PRA). So Refer to the removal procedure of Power Relay Assembly (PRA).

Installation

Main Relay, Pre Charge Relay, Pre Charge Resistor, Battery Current Sensor, High Voltage Battery Heater Relay and the High Voltage Battery Heater Fuse are integrated in the Power Relay Assembly (PRA). So Refer to the installation procedure of Power Relay Assembly (PRA).

##### Pre-charge Relay Schematic Diagrams

System Circuit Diagram With High Voltage Battery Heater System Without High Voltage Battery Heater System Circuit Diagram Without High Voltage Battery Heater System With High Voltage Batt ...

##### Pre-Charge Registor Specifications

Spectification ItemSpecificationCoilCapacity (W)60Resistance (?)30 ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Components and Components Location

Component 1. Battery Heater2. Battery Heater Relay3. Battery Heater Fuse4. Battery Heater Temperature Sensor ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. Driver Airbag (DAB)2. Steering Wheel3. Clock Spring4. Seat Belt Pretensioner (BPT)5. Side Impact Sensor (SIS)6. Side Airbag (SAB)7. Passenger Airbag (PAB)8. Front Impact Sensor (FIS)9. Curtain Airbag (CAB)10. Supplemental Restraint System Control Module(SRSCM)11. Airbag Warning La ...
Copyright © www.ksoulev.com 2020-2021