- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body Side Moulding / Fender Garnish Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Body Side Moulding / Fender Garnish Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Take care not to scratch the body surface.

1. | Using a screwdriver or remover, remove the fender garnish (A).

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Roof Side Moulding Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### A Pillar Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Adjustment 1. After loosening the hinge (A) mounting bolt, adjust the hood (B) clearance by moving it up and down, or left and right. 2. Adjust the hood height by turning the hood overslam bumpers (C). 3. After loosening the hood latch (D) mounting bolts, adjust the latch by moving it up ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cowl Side Trim Components and Components Location

Component Location 1. Cowl side trim ...
Copyright © www.ksoulev.com 2020-2021