- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Blower / PWM Blower Module Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Blower / PWM Blower Module Repair procedures

Inspection

1. | Turn the ignition switch OFF.

2. | Manually operate the control switch and measure the voltage of blower motor.

3. | Select the control switch to raise voltage until high speed.

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the glove box housing. (Refer to Body - "Glove Box Housing")

3. | Disconnect the connector (A) and then remove the blower resistor (B) after loosening the mounting screws.

4. | Install in the reverse order of removal.

##### Blower Motor Repair procedures

Inspection 1. Connect the battery voltage and check for the blower motor rotation. 2. If the blower motor voltage does not operate well, substitute with a verified blower motor and check for p ...

##### Climate Control Air Filter Description and Operation

Description The climate control air filter is located in the blower unit. It eliminates foreign materials and odor. The particle filter performs a role as an odor filter as well as a conventio ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the rear door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m, 12.3 ~ 15.9 lb-ft) 2. Detach the clips, then remove the rear door side weatherstrip (A). 3. Install in the reverse order of removal. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cowl Side Trim Components and Components Location

Component Location 1. Cowl side trim ...
Copyright © www.ksoulev.com 2020-2021