- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Seat Belt Pretensioner / Seat Belt Pretensioner (BPT) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / Seat Belt Pretensioner / Seat Belt Pretensioner (BPT) Repair procedures

Removal

1. | Disconnect the battery negative cable, and wait for at least thirty seconds before beginning to work.

2. | To remove the emergency fastening device (C), keep on pushing the lock pin (A) as arrow direction. And then remove the seat belt after pushing the lock pin (B).

3. | Remove the center pillar lower trim. (Refer to Body - "Center pillar trim")

4. | Remove the center pillar upper trim. (Refer to Body - "Center pillar trim")

5. | After loosening the mounting bolt, remove the front seat belt upper anchor (A).

6. | Disconnect the seat belt pretensioner connector (A).

7. | Loosen the seat belt pretensioner mounting bolt (B) and remove the seat belt pretensioner.

Installation

1. | Remove the ignition key from the vehicle.

2. | Disconnect the battery negative cable and wait for at least thirty seconds.

3. | Install the seat belt pretensioner with bolt (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

4. | Connect the seat belt pretensioner connector (A).

5. | Install the front seat belt upper anchor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

6. | Install the center pillar upper trim. (Refer to Body - "Center pillar trim")

7. | Install the center pillar lower trim. (Refer to Body - "Center pillar trim")

8. | Insert the seat belt to the emergency fastening device (A).
Make sure that the lock pin is connected properly.

9. | Reconnect the battery negative cable.

10. | After installing the seat belt pretensioner, confirm proper system operation:
• | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.

##### Seat Belt Pretensioner (BPT) Components and Components Location

Components ...

##### Emergency Fastening Device (EFD) Description and Operation

Description Emergency Fastening Device (EFD) is deployed concurrently with the Belt Pretensioner to strongly pull down the seat belt during a deployment condition after a collision. It is locat ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Function Of Safety Power Window When driver door power window auto-up switch is operated, safety function is activated. 1. Safety function condition If a force of 100N or over is detected (using a 10N/mm spring) while pulling up the window, the window automatically reverses and pulls down. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Hub - Carrier Components and Components Location

Components 1. Rear dust cover2. Rear wheel hub assembly3. Rear brake disc ...
Copyright © www.ksoulev.com 2020-2021