- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Windows / Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Power Windows / Description and Operation

Function Of Safety Power Window

When driver door power window auto-up switch is operated, safety function is activated.

1. | Safety function condition If a force of 100N or over is detected (using a 10N/mm spring) while pulling up the window, the window automatically reverses and pulls down.

2. | Reversing distance of window (not activated when holding the auto-up switch)
– | When a jamming object is detected between 4mm - 250mm from top of the door. > Window reverses and pulls down to 300mm from top of the door.
– | When a jamming object is detected over 250mm from top of the door. > Window reverses and pulls down to 20mm from jamming position.

3. | Reversing distance of window (while holding the auto-up switch)
– | When a jamming object is detected while holding the auto-up switch. > Window reverses and pulls down to 25mm from jamming position.
– | Auto-up function is not available during the 5 seconds from the above condition > When holding the auto-up switch, window operates in the manual-up mode. (Safety function is not activated.)
– | When holding the auto-up switch after 5 seconds from the above condition. > Window reverses and pulls down to 25mm from jamming position.

4. | Safety function deactivated area Safety function is not available in 4mm from top of the door.

Initializing Method Of The Safety Power Window

1. | Initializing Battery Connection When battery power is removed for over 5 minutes, safety power window switch needs to be initialized.
(1) | Pre-initializing operation of power window
– | Manual-Up/Down function is available
– | Auto-Up function is not available (When holding the auto-up/down switch, window operates in manual-up/down mode.)
(2) | Initializing method When the window is open, close the window by holding the switch until it is fully closed and keep it closed for at least 0.2 second. (Initialization may fail if the procedure is started when the window is fully closed.)
(3) | If the initializing state of the safety power window is in jammed status, the following condition may occur:
– | Safety function is not available.

2. | Initializing fail safe mode
(1) | If the window is moved by compulsion or if the motor has a problem, the power window switch may enter the fail safe mode for user''s safety.
(2) | Power window operation in fail safe mode
– | Auto/Manual-Down function is available
– | Auto/Manual-Up function is not available (When auto/manual-up is operated, the window rises only 20mm and stops moving.)

##### Components and Components Location

Component Location 1. Drive power window switch2. Passenger power window switch3. Front window motor4. Rear window motor5. Rear window switch ...

##### Power Window Motor Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Electric A/C compressor Components and Components Location

Components Location [Without Heat Pump] 1. Electric A/C compressor [With Heat Pump] 1. Electric A/C compressor Components 1. Control Part2. Motor Part3. Compression Part ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Luggage Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Using a screwdriver or remover, remove the luggage lamp (A). 3. Remove the luggage lamp (A) after disconnecting the connector (B). Installation 1. Install the luggage lamp assembly after connecting the lamp connector. ...
Copyright © www.ksoulev.com 2020-2021