- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Auto Lighting Control System / Auto Light Sensor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Auto Lighting Control System / Auto Light Sensor Repair procedures

Inspection

In the state of IGN1 ON, when the multi function switch module detects auto light switch on, tail lamp relay output and head lamp low relay output are controlled according to auto light sensor''s input.
During IGN1 ON, the BCM monitors the range of this supply and alerts the failure as soon as the supply''s voltage is out of range. When this failure occurs and persists, the head lamp must be turned on regardless of the sunlight level detected by the sensor.
This is designed to prevent any head lamp cut off when the failure occurs during the night.

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the photo & auto light sensor (A) from crash pad upper side by using screw (-) driver.

3. | Remove the auto light connector (B).

Installation

1. | Reconnect the auto light connector.

2. | Install the auto light sensor.

##### Auto Light Switch Repair procedures

Inspection 1. Operate the auto light switch, then check for continuity between terminals of multi-function switch connector. ...

##### AVN System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Panorama sunroof2. Panorama sunroof switch3. Panorama sunroof motor & controller4. Roller blind motor & slave controller ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Brake Pedal Repair procedures

Removal 1. Turn ignition switch OFF and disconnect the negative (-) battery cable. 2. Remove the crash pad lower panel and reinforcing panel. (Refer to the Body group - crash pad) 3. Remove the lower duct (A). 4. Pull down steering column shaft after removing bolts and nuts. (Re ...
Copyright © www.ksoulev.com 2020-2021