- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: AHB(Active Hydraulic Boost) System / Brake Line Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / AHB(Active Hydraulic Boost) System / Brake Line Repair procedures

Removal

1. | Disconnect the brake fiuid level switch connector, and remove the reservoir cap.

2. | Remove the brake fluid from the master cylinder reservior with a syringe.
Do not spill brake fluid on the vehicle as it may damage the paint. If brake fluid comes in contact with the paint, wash off immediately with water.

3. | Remove the wheel & tire.
Tightening torque : 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

4. | Remove the brake hose mounting bracket bolt (A).

5. | Disconnect the brake tube by loosening the tube flare nut (B).
Tightening torque: 12.7 ~ 16.7 N.m (1.3 ~ 1.7 kgf.m, 9.4 ~ 12.3 lb-ft)
Front Rear

6. | Remove the brake hose clip (A).

7. | Disconnect the brake hose from the brake caliper by loosening the bolt (A).
Tightening torque: 24.5 ~ 29.4 N.m (2.5 ~ 3.0 kgf.m, 18.1 ~ 21.7 lb-ft)
Front Rear

Inspection

1. | Check the brake tubes for cracks, crimps and corrosion.

2. | Check the brake hoses for cracks, damage and fluid leakage.

3. | Check the brake tube flare nuts for damage and fluid leakage.

4. | Check brake hose mounting bracket for crack or deformation.

Installation

1. | Install in the reverse order of removal.
Use a new washer (A) whenever installing.

2. | After installation, bleed the brake system. (Refer to Brake system bleeding)

3. | Check for brake fluid leaks.

##### Brake Line Components and Components Location

Components ...

##### Brake Pedal Components and Components Location

Components 1. Brake pedal stroke sensor2. Stop lamp switch3. Brake pedal ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Glass Defogger Printed Heater Repair procedures

Inspection Wrap tin foil around the end of the voltmeter test lead to prevent damaging the heater line. Apply finger pressure on the tin foil, moving the tin foil along the grid line to check for open circuits. 1. Turn on the defogger switch and use a voltmete ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Door Latch Components and Components Location

Component Location 1. Front door latch ...
Copyright © www.ksoulev.com 2020-2021