- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Steering wheel / Heated Steering wheel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Steering System / Steering wheel / Heated Steering wheel Repair procedures

Inspection

1. | Measure a resistance of NTC and Heated pad.
– | NTC resistance(Yellow / Black) - 10k? (9k? ~ 11k?), 25°C
– | Heated pad resistance (Yellow , Black) - 1.73? ( 2.1 ~ 2.5 ? )

2. | Measure a temperature.
– | The temperature of wheel surface grip must rise from -20°C to 20°C within 6 minute
– | The temperature of wheel surface grip must keep 38°C ± 4°C after 25 minute
– | Temperature measurement points (1~8)

##### Heated Steering wheel Schematic Diagrams

System Circuit Diagram ...

##### Flex Steer Components and Components Location

Components Location 1. Flex steering swithch ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Hub / Knuckle Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) Be careful not to da ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Latch Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...
Copyright © www.ksoulev.com 2020-2021