- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Air Conditioning System / Evaporator Temperature Sensor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Air Conditioning System / Evaporator Temperature Sensor Repair procedures

Inspection

1. | Turn the ignition switch OFF.

2. | Disconnect the evaporator temperature sensor connector.

3. | Measure the resistance between terminals "1" and "2" of the evaporator temperature sensor.

4. | Connect the evaporator temperature sensor connector.

5. | Run the engine and turn the A/C switch ON, then measure the voltage between the terminals of the harness connector. Specification
Evaporator core temperature[°C(°F)] | Resistance[K?]
-10 / (14) | 43.35
0 / (32) | 27.62
10 / (50) | 18.07
20 / (68) | 12.11
30 / (86) | 8.3
40 / (104) | 5.81

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the console side cover (A). [RH]

3. | Disconnect the evaporator temperature sensor connector (A).

4. | Remove the evaporator temperature sensor (A) by pulling it out after rotating it 90° in a counterclockwise direction.

5. | Install in the reverse order of removal.

##### Evaporator Temperature Sensor Description and Operation

Description The evaporator temperature sensor will detect the evaporator core temperature and interrupt compressor relay power in order to prevent evaporator from freezing by excessive cooling ...

##### In-car Sensor Description and Operation

Description The In-car air temperature sensor is integrated into the heater & A/C control unit. The sensor contains a thermistor which measures the temperature of the inside. The signal deci ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Latch Release Handle Components and Components Location

Component Location 1. Hood latch release handle ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Instrument Cluster Components and Components Location

Components Connector Pin Information No.DescriptionNo.Description1Ground signal 3 (Power ground)21Trip switch (-) input2Illumination output (-)22Trip switch 1 (+) input(Trip button)3Rheostat switch down input23Trip switch 2 (+) input(Cruise button)4Rheostat switch up input24-5Detent output (+) ...
Copyright © www.ksoulev.com 2020-2021