- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Seat Belt Buckle Switch (BS) Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Seat Belt Buckle Switch (BS) Description and Operation

Description

The SRSCM shall monitor the status of the driver and front passenger seat belt buckle. The SRSCM provides one pin each for the driver and front passenger seat belt buckle status input. The seat belt buckle circuit operates from internal boost voltage supplied by the SRSCM, and uses chassis ground for the signal return. The buckle status shall modify the SRSCM deployment. If the buckle status is unbuckled, the corresponding pretensioner will not be deactivated.

##### Side Impact Sensor (SIS) Repair procedures

Removal Pressure Side Impact Sensor • Removal of the airbag must be performed according to the precautions / procedures described previously. • ...

##### Seat Belt Buckle Switch (BS) Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Cushion Cover Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Driver power window main switch2. BCM (Body Control Module)3. Door lock switch4. Front door lock actuator & switch5. Rear door lock actuator & switch6. Tailgate lock actuator & switch ...
Copyright © www.ksoulev.com 2020-2021