- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Keyless Entry / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Keyless Entry / Specifications

Specification

Item | Specification
Rated voltage | DC 3V
Operating voltage | DC 2.7V ~ 3.3V
Operating temperature | -20°C ~ +60°C (-4°F ~ +140°F)
RF Modulation | FSK
LF Modulation | ASK
RF frequency | 433.92 MHz
Battery | CR2032 (3V / 1EA)
Transmissible distance | 30m or more
Battery lifetime | 2 years or more (at 20 times per day)
Number of buttons | 3
Function | Door lock
Door unlock
Tailgate open

##### Keyless Entry

...

##### Components and Components Location

Component Location 1. BCM & RF receiver2. Key warning switch3. Front door lock actuator & switch4. Rear door lock actuator & switch5. Tailgate open switch ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Current Sensor Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Prcedure") 3. Remove the high voltage battery system assembly. (Refer to High Voltage Battery System - Repair procedures - "Removal") 4. Remove the hi ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Replacement • Be careful not to damage the fender and body. • When removing the clips, use a clip remover. 1. Remove the head lamps. (Refer to Body Electrical System - "Head Lamps") 2. Remove the A pilla ...
Copyright © www.ksoulev.com 2020-2021