- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Airbag Module / Curtain Airbag (CAB) Module Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / Airbag Module / Curtain Airbag (CAB) Module Repair procedures

Removal

1. | Disconnect the battery negative cable and wait for at least thirty seconds before beginning to work.

2. | Remove the roof trim assembly. (Refer to Body - "Roof trim assembly")

3. | Disconnect the curtain airbag harness connector (A).

4. | After loosening the mounting bolts and nuts remove the curtain airbag.

Installation

1. | Remove the ignition key from the vehicle.

2. | Disconnect the battery negative cable and wait for at least thirty seconds.

3. | Tighten the curtain airbag mounting bolts and nuts.
Tightening torque Bolt : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft) Nut : 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)
• | Never twist the airbag module during installation as twisted module may result in abnormal operation. (of the airbag module.)

4. | Connect the curtain airbag connector.

5. | Install the roof trim assembly. (Refer to Body - "Roof trim assembly")

6. | Reconnect the battery negative cable.

7. | After installing the curtain airbag (CAB), confirm proper system operation:
• | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.

##### Curtain Airbag (CAB) Module Components and Components Location

Components ...

##### Airbag Module Disposal Description and Operation

Airbag Disposal Special tool required Deployment tool 0957A-34100A Before scrapping any airbags or side airbags (including those in a whole vehicle to be scrapped), the airbags or side airba ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Port Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Parking Assist Sensor Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the front/rear bumper cover. (Refer to Body - "Front Bumper Cover") (Refer to Body - "Rear Bumper Cover") 3. Disconnect the connector (A) from the ultrasonic sensor. [Front sensor, Rear center sensor] [Rear side senso ...
Copyright © www.ksoulev.com 2020-2021