- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Axle Assembly / Rear Hub - Carrier Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Driveshaft and axle / Rear Axle Assembly / Rear Hub - Carrier Repair procedures

Replacement

1. | Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported.

2. | Remove the rear wheel and tire (A) from rear hub.
Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

3. | Loosen the guide rod bolt (B) and the remove the rear caliper body (A).
Tightening torque: 21.6 ~ 31.4 N.m (2.2 ~ 3.2 kgf.m, 15.9 ~ 23.1 lb-ft)

4. | Remove the pads (B), in the caliper carrier (A).

5. | Remove the brake caliper mounting bolts (B), and then place the brake caliper assembly (A) with wire.
Tightening torque: 63.7 ~ 73.5 N.m (6.5 ~ 7.5 kgf.m, 47.0 ~ 54.2 lb-ft)

6. | Disconnect the wheel speed sensor connector (A).

7. | Loosen the screws (B), and then remove the brake disc (A).
Tightening torque: 4.9 ~ 5.8 N.m (0.5 ~ 0.6 kgf.m, 3.6 ~ 4.3 lb-ft)

8. | Loosen the bolts and then remove the hub bearing (A).
Tightening torque: 49.0 ~ 58.8 N.m (5.0 ~ 6.0 kgf.m, 36.2 ~ 43.3 lb-ft)

9. | Remove the hub bearing by using the rubber hammer.

10. | Install in the reverse order of removal.

Inspection

1. | Check the hub for cracks and the splines for wear.

2. | Check the brake disc for scoring and damage.

3. | Check the rear axle carrier for cracks.

4. | Check the bearing for cracks or damage.

Installation

1. | Install in the reverse order of removal
Use a SST (09581-11000) when installing the brake caliper assembly. (Refer to Brake System - "Front Disc Brake")

2. | Check the front alignment. (Refer to Suspension System - "Front Alignment")

##### Rear Hub - Carrier Components and Components Location

Components 1. Rear dust cover2. Rear wheel hub assembly3. Rear brake disc ...

##### Suspension System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Ambient Temperature Sensor Description and Operation

Description The ambient temperature sensor is located at the front of the condenser and detects ambient air temperature. It is a negative type thermistor; resistance will increase with lower temperature, and decrease with higher temperature. The sensor output will be used for discharge tem ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Glove Box Housing Components and Components Location

Component Location 1. Glove box housing ...
Copyright © www.ksoulev.com 2020-2021