- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Smart Key System / Smart Key Unit Components and Components Location

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Smart Key System / Smart Key Unit Components and Components Location

Component (1)

Connector Pin Information

No. | Connector A | Connector B | Connector C
1 | V_BAT CPU | Assistant side antenna ground | Immobilizer antenna ground
2 | V_BAT Load | Assistant side antenna power | Immobilizer antenna power
3 | Ignition 1 | Driver side antenna ground | -
4 | Ignition 2 relay | Driver side antenna power | -
5 | Ignition 1 relay | Wheel speed | -
6 | - | P position | SSB LED ON
7 | - | - | SSB LED ACC
8 | EMS COM | C CAN low | SSB illumination power
9 | - | C CAN high | -
10 | B CAN high | Interior 1 antenna ground | -
11 | B CAN low | Interior 1 antenna power | -
12 | ACC | Bumper antenna ground | -
13 | Ignition 2 | Bumper antenna power | Stop lamp fuse
14 | ACC relay | Interior 2 antenna ground | Brake switch
15 | Starter relay | Interior 2 antenna power | -
16 | Start feedback | - | Immobilizer indicator
17 | ESCL battery | RPM | Exterior buzzer
18 | - | - | SSB illumination ground
19 | - | SSB switch 2 | ?
20 | Assistant toggle button | SSB switch 1
21 | Driver toggle button | ?
22 | -
23 | Power ground 2
24 | Power ground 1

##### Smart Key Repair procedures

Inspection 1. Check that the red light flickers when the door lock or unlock button is pressed on the transmitter. 2. Remove the battery (A) and check voltage if the red light doesn''t flicker ...

##### Smart Key Unit Schematic Diagrams

Circuit Diagram ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Shield Inner Cover Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Door Opener Actuator Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the front bumper cover. (Refer to Body - "Front Bumper Cover") 3. Remove the charge door opener cover assembly. (Refer to Body - "Charge Door Opener Cover") 4. Remove the charge door opener actuator cable (A). 5. ...
Copyright © www.ksoulev.com 2020-2021