- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body Side Moulding / Front Wheel Guard Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Body Side Moulding / Front Wheel Guard Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Take care not to scratch the body surface.

1. | Remove the front tire.

2. | After loosening the mounting clips and screws, remove the front wheel guard (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### A Pillar Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Rear Wheel Guard Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Drive power window switch2. Passenger power window switch3. Front window motor4. Rear window motor5. Rear window switch ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Audio Remote Control Repair procedures

Inspection 1. Check for resistance or output voltage between terminals in each switch position. [Audio] SwitchConnector terminalResistance (±5%)Output voltageSeek up2-4430 ?0.4 V ± 0.22Seek down2-41.1 k?1.0 V ± 0.22Mode2-42.11 k?1.5 V ± 0.22Mute2-43.11 k?2.0 V ± 0.22Volume up2-44.61 k?2 ...
Copyright © www.ksoulev.com 2020-2021