- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Seat / Rear Seat Back Cover Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Seat / Rear Seat Back Cover Repair procedures

Replacement

[LH]

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear seat back assembly [LH]. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Push the lock pin (B), remove the rear seat headrest (A).

3. | Using a screwdriver or remover, remove the rear seat folding bezel (A).

4. | Using a screwdriver or remover, remove the rear seat belt center cover (A).

5. | Using a screwdriver or remover, remove the tether anchor garnish (A).

6. | Using a screwdriver or remover, remove the rear seat back bush hinge (A).

7. | Remove the protector (A) located in the bottom side of the rear seat back.

8. | Zip off the rear seat back cover located in the side (A), and then pull it up.

9. | Pull out the hooks (A) by the rear seat back frame.

10. | Turn the rear seat back cover inside out. Then pull out the headrest guides (A) while pinching both sides of the lower part of the guides, and remove them.

11. | Remove the rear seat back cover (A) from the rear seat back frame (B).

12. | Remove the hog-ring clip (A) velcro tape (B) on the rear of seat back and then remove the rear seat back cover (C).

13. | Install in the reverse order of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hog-ring clips (A).
• | Replace the hog-ring clips with new ones using special tool (C) (09880-4F000).

[RH]

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear seat back assembly [RH]. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Push the lock pin (B), remove the rear seat headrest (A).

3. | Using a screwdriver or remover, remove the rear seat folding bezel (A).

4. | Using a screwdriver or remover, remove the tether anchor garnish (A).

5. | Using a screwdriver or remover, remove the rear seat back bush hinge (A).

6. | Remove the protector (A) located in the bottom side of the rear seat back.

7. | Zip off the rear seat back cover located in the side (A), and then pull it up.

8. | Pull out the hook (A) by the rear seat back frame.

9. | Turn the rear seat back cover inside out. Then pull out the headrest guides (A) while pinching both sides of the lower part of the guides, and remove them.

10. | Remove the rear seat back cover (A) from the rear seat back frame (B).

11. | Removing the hog-ring clips (A), Velcro tape (B) on the rear of seat back and then remove the seat back cover (C).

12. | Install in the reverse order of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hog-ring clips (A).
• | Replace the hog-ring clips with new ones using special tool (C) (09880-4F000).

##### Rear Seat Back Cover Components and Components Location

Component Location 1. Rear seat back cover [LH]2. Rear seat back cover [RH] ...

##### Rear Seat Cushion Cover Components and Components Location

Component Location 1. Rear seat cushion cover ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hands Free Switch Repair procedures

Inspection 1. Check for resistance between terminals in each switch position. [Voice + Bluetooth] [Voice + Bluetooth] SwitchConnector terminalResistance (±5%)Output voltage (± 0.22)Voice2-410.71 k?3.5 V ± 0.22Call off2-418.91 k?4.0 V ± 0.22Call2-440.91 k?4.5 V ± 0.22 Removal 1. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Driver power window main switch2. BCM (Body Control Module)3. Door lock switch4. Front door lock actuator & switch5. Rear door lock actuator & switch6. Tailgate lock actuator & switch ...
Copyright © www.ksoulev.com 2020-2021