- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Cowl Top Cover / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Cowl Top Cover / Repair procedures

Replacement

1. | Remove the cap (A), the nuts and the wiper arm (B).
Tightening torque : 22.6 ~ 26.5 N.m(2.3 ~ 2.7 kgf.m, 16.6 ~ 19.5 lb-ft)

2. | Remove the glue from both ends (A) of the hood weatherstrip.

3. | Disconnect the cowl top cover nozzle hose (A).

4. | Detach the clips, then remove the cowl top cover (A).

5. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Components and Components Location

Component Location 1. Cowl top cover ...

##### Crash Pad

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Pillar Trim Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Center Pillar Trim Components and Components Location

Component Location 1. Center pillar lower trim2. Center pillar upper trim ...
Copyright © www.ksoulev.com 2020-2021