- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Steering wheel / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Steering System / Steering wheel / Repair procedures

Replacement

1. | Disconnect the battery negative cable from the battery and then wait for at least 30 seconds.

2. | Turn the steering wheel so that the front wheels are facing straight ahead.

3. | Remove the airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring")

4. | Disconnect the connector & lock nut (A) and then remove the steering wheel using the special service tool (09561-11001).
Tightening torque : 39.2 ~ 49.0N-m (4.0 ~ 5.0kgf-m, 28.9 ~ 36.2lb-ft)
• | Do not use a hammer when removing the steering wheel as it may damage the steering column.
• | Do not reuse lock nuts.
• | Lock nuts must be replaced with new ones when assembling. (SEAL-LOCK has been processed)

5. | Install in the reverse order of removal.

Disassembly

1. | Loosen the screw (A-6ea) and then remove the lower cover (B) from the steering wheel body.

2. | Remove the wiring (A) & Heated unit (B).

3. | Remove the remote control upper switch assembly (A) and wiring.

4. | Loosen the screw and then remote control switch assembly (A).

5. | Installation is the reverse of the removal.

##### Components and Components Location

Component 1. Airbag module 2. Remote control upper switch 3. Remote control lower switch 4. Steering wheel assembly 5. Heated unit 6. Wiring 7. Steering wheel lower cover ...

##### Heated Steering wheel Description and Operation

Description When manually selected, the heated steering wheel system improves the thermal comfort of the driver by heating the steering wheel. 1. Heate control unit 2. Heated pad Specifi ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Smart Key Unit Repair procedures

Inspection Smart Key Unit – Refer to Smart key System - "Smart key Diagnostic" Smart Key Switch – Refer to Smart key System - "Smart key Diagnostic" Antenna – Refer to Smart key System - "Smart key Diagnostic" Trunk Lid Open Switch 1. Check for continuity ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Component Replacement after Deployment Before doing any SRS repairs, use the GDS to check for DTCs. Refer to the Diagnostic Trouble Code list for repairing of the related DTCs. When the front airbag(s) deployed after a collision, replace the following items. ...
Copyright © www.ksoulev.com 2020-2021