- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tire Pressure Monitoring System / Troubleshooting

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Tire Pressure Monitoring System / Troubleshooting

TPMS Inspection method

Inspection

Find the inspection number by referring to the table above. The following content is irrelevant of the inspection procedure.

1. | Warning lamp types
• | Keeps on without blinking : Low pressure tire warning lamp
• | Flashes at 0.5 second intervals constantly : Initial state warning lamp
• | Cluster blinks for 1 minute at 1 second intervals, then turns ON : Error code warning lamp
Turn IG OFF and then IG ON again to check the warning light type.

2. | (1) Check the warning lamp state.
• | Check the vehicle warning lamp state.
• | Check if the warning lamp state is caused by tire low pressure. Symptom : Keeps on without blinking

3. | (2) Check the warning lamp state.
• | Check the vehicle warning lamp state.
• | Check if the warning lamp state is caused by the initial state (virgin mode) of TPMS receiver. Symptom : Flashes at 0.5 second intervals constantly.

4. | (3) Check the warning lamp state.
• | Check the vehicle warning lamp state.
• | Check if the warning lamp state is caused by error code (TPMS receiver & TPMS sensor failure). Symptom : Cluster blinks for 1 minute at 1 second intervals, then turns ON.

5. | Low tire pressure warning lamp Cold : Vehicle kept for more than 60 minutes after stopping. > 0.07 kgf/cm? (1.0 psi) additional injection at the specified tire pressure. Hot : Driven vehicle > 0.28 kgf/cm? (4.0 psi) additional injection at the specified tire pressure.
In case the warning lamp fails to turn OFF after injecting tire pressure, disconnect the GDS and drive less than 1 km at 25 km/h.

6. | Inspect initial state warning lamp
A. | TPMS warning lamp (1) Check the TPMS warning lamp status. (2)Flashes at 0.5 second intervals constantly. -> Initial state warning lamp
Turn IG OFF and then IG ON again to check the warning lamp type.
B. | Items to check in case of blinking warning lamp (1). Enter sensor ID. (Refer to TPMS Receiver - "Repair procedures") (2). Enter vehicle name. (Refer to TPMS Receiver - "Repair procedures") (3). Enter VIN. (Refer to TPMS Receiver - "Repair procedures") (4). Change TPMS ECU mode (to Standard mode).

7. | DTC checklist for performance test.
List | symptoms | Inspection items | Detailed checklist | Component/parts
C1312(FL) C1313(FR) C1314(RL) C1315(RR) | TPMS sensor receive error. | Sensor RF transmission state | Confirm sensor RF transmission Check sensor DTC Inspect Ssnsor battery | TPMS Sensor Vehicle electronic units noise Vehicle operating conditions
C1332(FL) C1333(FR) C1334(RL) C1335(RR) | Sensor internal failure | Inspect sensor RF transmission Sensor battery voltage | Check sensor RF transmission Check sensor battery (GDS) | TPMS Sensor
C1662 | Auto learning failure | Sensor RF transmission state Inspect EMS vehicle speed (VS) Inspect vehicle noise | Confirm sensor RF transmission Inspect sensor battery Inspect EMS vehicle speed (VS) Inspect vehicle electronic unit noise | TPMS Sensor Vehicle electronic units noise Vehicle operating condition EMS vehicle speed signal
C1663 | Auto learning failure | Sensor RF transmission state Inspect EMS vehicle speed (VS) Inspect vehicle noise | Confirm sensor RF transmission Inspect sensor battery Inspect EMS vehicle speed (VS) Inspect vehicle electronic unit noise | TPMS Sensor Vehicle electronic units noise Vehicle operating condition EMS vehicle speed signal
• | Be sure to check DTC. (Refer to DTC manual - "Tire Pressure Monitoring")
• | If the TPMS warning light does not turn on : TPMS sensor periodically learns the sensor through driving.
• | If the TPMS warning light turns on : Replace TPMS sensor, TPMS receiver.

##### Description and Operation

Description TREAD Lamp – Tire Under Inflation / Leak Warning. 1. Turn on condition • When tire pressure is below allowed threshold • When rapid leak is detected ...

##### TPMS Sensor Description and Operation

Description Mode of Operation ASIC Mode 1. Factory Mode The factory mode is the mode that allows the TPM sensor to transmit RF Frames and sample LF more often in the HKMC factory. The TPM ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. Front seat headrest2. Front seat headrest guide3. Front seat back cover4. Front seat back heater5. Front seat back pad6. Front seat back lumbar assembly7. Front seat back frame assembly8. Front seat back board9. Front seat cushion cover10. Front seat cushion heater11. Front seat c ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Drive power window switch2. Passenger power window switch3. Front window motor4. Rear window motor5. Rear window switch ...
Copyright © www.ksoulev.com 2020-2021