- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body (Interior and Exterior) / Rear Door

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door

- Components and Components Location
- Repair procedures
- Rear Door Trim Components and Components Location
- Rear Door Trim Repair procedures
- Rear Door Inside Handle Repair procedures
- Rear Door Window Glass Components and Components Location
- Rear Door Window Glass Repair procedures
- Rear Door Module Components and Components Location
- Rear Door Module Repair procedures
- Rear Door Outside Handle Components and Components Location
- Rear Door Outside Handle Repair procedures
- Rear Door Latch Components and Components Location
- Rear Door Latch Repair procedures
- Rear Door Belt Outside Weatherstrip Repair procedures
- Rear Door Belt Inside Weatherstrip Repair procedures
- Rear Door Side Weatherstrip Repair procedures

##### Rear Bumper Beam Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Components and Components Location

Components (1) 1. Rear door pull cap2. Rear door inside handle cap3. Rear door delta inner cover4. Rear door trim5. Rear door belt inside weatherstrip6. Rear door panel7. Rear door delta garnish ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tire Repair procedures

Tire Wear 1. Measure the tread depth of the tires. Tread depth [limit] : 1.6 mm (0.0630 in.) 2. If the remaining tread depth (A) is less than the limit, replace the tire. When the tread depth of the tires is less than 1.6 mm(0.063 in), the wear indicators ( ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Hub - Carrier Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the rear wheel and tire (A) from rear hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) 3. Loosen the guide rod bolt (B) and the remove ...
Copyright © www.ksoulev.com 2020-2021