- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Battery Temperature Sensor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Battery Temperature Sensor Repair procedures

Installation

Battery temperature sensor can not be disassembled.

1. | Turn the ignition switch OFF.

2. | Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure")

3. | Remove the high voltage battery system assembly. (Refer to High Voltage Battery System - Repair procedures - "Removal")

4. | Remove the high voltage battery pack upper case. (Refer to High Voltage Battery System - Case - "Upper Case")

5. | Connect the SST (No: 0K918-E4100, 0K375-E4100, 0K375-E4200) as shown in the image below.

6. | Connect the GDS to DLC.

7. | Turn the ignition switch ON.

8. | Check the "Battery Module Temperature" in the GDS service data.

9. | Turn the ignition swtich OFF.

10. | Disconnect the SST (high votlage battery cable & BMS terminal).

11. | Check resistance for each temperature sensor.
Temperature (°C) | Resistance (K?) | Tolerance (%)
-40 | 204.5 | ±4.0
-30 | 117.8 | ±3.5
- 20 | 70.34 | ±3.0
- 10 | 43.43 | ±2.5
0 | 27.63 | ±2.0
10 | 18.07 | ±1.6
20 | 12.11 | ±1.2
30 | 8.303 | ±1.2
40 | 5.813 | ±1.5
50 | 4.149 | ±1.9
60 | 3.013 | ±2.2
70 | 2.225 | ±2.5

##### Battery Temperature Sensor Schematic Diagrams

Circuit Diagram ...

##### Runaway Arresting Device (RAD) Specifications

Specification ItemSpecificationRemarkRAD Combined Resistance (?)Less than 3 (20°C)Checkable by multi testerRAD Terminal Resistance (?)Less than 0.375 (20°C)Checkable by multi testerRAD Switch P ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hands Free Switch Repair procedures

Inspection 1. Check for resistance between terminals in each switch position. [Voice + Bluetooth] [Voice + Bluetooth] SwitchConnector terminalResistance (±5%)Output voltage (± 0.22)Voice2-410.71 k?3.5 V ± 0.22Call off2-418.91 k?4.0 V ± 0.22Call2-440.91 k?4.5 V ± 0.22 Removal 1. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Trim Components and Components Location

Component Location 1. Tail gate trim ...
Copyright © www.ksoulev.com 2020-2021