- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Roof Trim / Roof Trim Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Roof Trim / Roof Trim Assembly Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear seat assembly. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Remove both sides of the front pillar trim. (Refer to Interior Trim - "Front Pillar Trim")

3. | Remove both sides of the canter pillar upper trim. (Refer to Interior Trim - "Center Pillar Trim")

4. | Remove both sides of the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim")

5. | Remove both sides of the sunvisor and retainer. (Refer to Roof Trim - "Sunvisor")

6. | Remove both sides of the assist handle. (Refer to Roof Trim - "Assist Handle")

7. | Remove the overhead console lamp. (Refer to Body Electrical System - "Overhead Console Lamp")

8. | Remove the room lamp. (Refer to Body Electrical System - "Room Lamp")

9. | Tilt the front seat back towards the rear of the vehicle as far as possible.

10. | Remove the ECM mirror cover (A).

11. | Disconnect the ECM mirror connector (B).

12. | Remove the LDWS cover (A).

13. | Disconnect the LDWS unit connector (A).

14. | Disconnect the roof trim main connector (A) and the mounting clips (B) in the front pillar. [Driver''s] [Passenger''s]

15. | Using a clip remover, detach the roof trim assembly mounting clips (A).

16. | Slighty remove the tail gate weatherstrip.

17. | Slightly lower the rear side of the roof trim.

18. | To remove the roof trim, press the lock pin (A) in the direction of the arrow.

19. | Before removing the roof trim, slightly lower the roof trim and disconnecting the roof antenna connectors (A).

20. | Remove the roof trim assembly (A) from the vehicle through the tail gate.

21. | Remove the vanity lamp. (Refer to Body Electrical System - "Vanity Lamp")

22. | Remove the hands free mic. (Refer to Body Electrical System - "Hands Free Mic")

23. | Remove roof trim wiring harness (A) from the roof trim assembly (B).
• | Take care not to damage the roof trim wiring harness (A) when removing.
1) | Apply the hot melt continuously when installing the roof trim wiring harness (A) on the roof trim (B) using the hot melt gun tool.
2) | Put anti-noise pad (C) on roof trim (B) to prevent the noise.

24. | Install in the reverse order of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damaged clips.

##### Roof Trim Assembly Components and Components Location

Component Location 1. Roof Trim Assembly ...

##### Tail Gate

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Side Airbag (SAB) Module Repair procedures

Removal The side airbag cannot be disassembled from the seat back assembly, so replace assembly when replacing the side airbag. 1. Disconnect the battery negative cable, and wait for at least thirty seconds before beginning to work. 2. Remove the front passen ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Latch Repair procedures

Replacement 1. Remove the charge door handle (A). 2. Loosen the front bumper upper cover mounting bolts and clips. 3. Gently lift the bumper upper cover. 4. Loosen the screw (B), and then remove the front bumper upper cover (A). 5. Loosen the bolts, and then remove the hood latch ...
Copyright © www.ksoulev.com 2020-2021