- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Air Conditioning System / Refrigerant line Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Air Conditioning System / Refrigerant line Repair procedures

Replacement

1. | Discharge refrigerant from refrigeration system.

2. | Replace faulty tube or hose.
• | Cap the open fittings immediately to keep moisture or dirt out of the system.

3. | Tighten joint of bolt or nut to specified torque.
• | Connections should not be tightened to over the specified torque.
Items | N.m | kgf.m | lb-ft
Compressor | 20.0 ~ 33.0 | 2.0 ~ 3.4 | 14.8 ~ 24.3
Accumulator mounting bolt | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Discharge hose mounting bolt
Discharge pipe mounting bolt
Suction pipe mounting bolt
Suction hose mounting bolt
Tube & Hose assembly mounting bolt
Accumulator nut | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Discharge hose nut
Discharge pipe nut
Suction pipe nut
Suction hose nut
Tube & Hose assembly nut
Refrigerant valve | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Chiller (Refrigerant line) | 5.9 ~ 9.8 | 0.6 ~ 1.0 | 4.3 ~ 7.2

4. | Evacuate air in the refrigeration system and charge system with refrigerant.
Specified amount Without heat pump : 550 ± 25g (19.4 ± 0.88 oz.) With heat pump : 900 ± 25g (31.7 ± 0.88 oz.)

5. | Inspect for leakage of refrigerant. Using a gas leak detector, check for leakage of refrigerant.

6. | Inspect A/C operation.

##### Refrigerant line Components and Components Location

Component Location [Without Heat Pump] 1. Refrigerant line [With Heat Pump] 1. Refrigerant line ...

##### Electric A/C compressor Specifications

Specification ModelESC33nMotorBLDC MotorControl TypeCANCompression TypeScrollCapacity33cc/revOperating Voltage Range190~320VRated Voltage288VMount TypeBracket Mounting, 4 Point Mounting ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Cowl top cover ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Pre-charge Relay Specifications

Specification ItemSpecificationONRated Voltage(V)450Rated Ampere(A)10Voltage Drop(V)Less than 0.5 (10A)CoilOperation Voltage(V)12Resistance(?)104.4 ~ 127.6 (20°C) ItemSpecificationRemarkMain Relay Switch (-) Resistance (?)?Checkable by multi testerPre Charger Relay Operation Sound"Click ...
Copyright © www.ksoulev.com 2020-2021